**the problemos.**

| complaint | how to fix | what you need | ✅ |
| --- | --- | --- | --- |
| tilt boi | Screw bfs  Tension differently | ⅝ inch screws  lock nuts | ✅ |
| can’t climb direct to center | Weight distribution (forward!)  I found a way but it’s risky with the time we have. We’d have to rearrange the lift post supports but if you drive this whole week and let me take the saturday with yoshiki it might work.  ...or i might take it home to work on | Wrench  Screwdriver  Cap | ✅ |
| Bent intake | Strengthen supports (use L’s?) |  |  |
| passive | Joseph? | Replaceeeee | ✅ |
| License plates | Make single-color plates |  | ✅ |
| Post supports |  |  | ✅ |
| Cap goes into robot | Antislip? |  | ✅ |
| Tipping | ………………nocando. |  | ✅ |
|  |  |  |  |